Installation instructions>

Click on the setup file in the ATSFixes folder to install ATSFixes.


The WILDLINK module is connected to the PC and is used as a wireless upload for GPS schedules, and wireless or remote downloading of data.

The USB driver will need to be installed, if the PC the WILDLINK will be used on cannot automatically install the driver.

Install Wildlink USB adaptor in CP210x_Universal_Windows folder

### Manual install ###

1. Using Windows File Explorer, locate the driver folder
   (that you previously unzipped)
2. Right click on the silabser.inf file and select Install
3. Follow the instructions

For additional information see "CP210x_Universal_Windows_Driver_ReleaseNotes.txt" 


When uploading a schedule to the logger from ATSFixes, swipe the magnet on the logger to activate the logger RF link.



When downloading data, pressing the "Download Data" tab requires a magnet swipe on the logger to activate the RF link.  


For remote downloading, the magnet does not need to be swiped on the logger.

For remote downloading, the logger will listen for a remote download command from the WILDLINK every 11 minutes.  
It is set for 11 minutes to prevent a download attempt during a scheduled GPS fix.  Just to keep them from occurring at the same time.


