ATS Elat Controller
-------------------------------------------------
Requirements
- This software is written to be compatible with all Windows PCs version 10 and up
- The hardware that interacts with this program requires at least one Type-A USB port
 
-------------------------------------------------
Installation
- To install the software, double click on Setup.exe
- Click past any warnings, and run through the installation steps
- The software should auto-open after installation
- For subsequent sessions of the software, search the start menu for "ATS ELAT Controller" and run the app from there.
- Desktop shortcuts for ease of access may be created if searching for the app on the start menu


-------------------------------------------------
Operation
- The interface scans for available COM ports on startup. Connect peripheral equipment to the PC before program startup
- There are two modes which are selectable in a dropdown menu. One is for only turning the tags on/off/locked on, and the other mode is for changing Pulse Rate Intervals.
- Please do not look directly into the UV LED on the activation device. This may cause damage to eyes.